**getPwm()**

**Description**

Get a joint’s current pulse width modulation (PWM) value. PWM has a resolution of 12-Bits, so PWM value can be from -4095 to +4095. If the value is bigger than 0, the joint turns clockwise. Smaller than 0, the joint turns counterclockwise.

**Syntax**

ArgonBase.ArgonJoint.getPwm()

or

ArgonArm.ArgonJoint.getPwm()

**Parameters**

None

**Returns**

*Int16\_t*: current pulse width modulation (PWM) value (-4095, +4095)

**Examples**